API Location					Method		Returns										Redirects to		Description			
---------------------------------------------------------------------------------------------------------------------


/api/																										API root
----------------


/api/v1/playback/																							Playback functions
----------------
/api/v1/playback/toggle				GET		JSON object														Toggle Playback
/api/v1/playback/play				GET		JSON object														Start playback
/api/v1/playback/pause				GET		JSON object														Pause playback
/api/v1/playback/next				GET		JSON object														Play next audio
/api/v1/playback/previous			GET		JSON object														Play previous audio
/api/v1/playback/info				GET		JSON object														Get the title, artist, album, path, type, ... of the current played resource

/api/v1/playlist/
----------------
/api/v1/playlist/get				GET		JSON object														Returns the whole current playlist
/api/v1/playlist/create             POST    JSON object                                                     Creates a playlist of the given directory
/api/v1/playlist/play               POST    JSON object                                                     Plays a playlist from the SD card

/api/v1/volume/
----------------
/api/v1/volume/up					GET		JSON object														Higher the volume (max. 20)
/api/v1/volume/down					GET		JSON object														Lower the volume (min. 0)
/api/v1/volume/mute					GET		JSON object														Mute (does not affect volume)
/api/v1/volume/unmute				GET		JSON object														Unmute (set volume to current volume)
/api/v1/volume/get					GET		JSON object														Do nothing, just get the volume
/api/v1/volume/<0-20>				GET		JSON object														Set volume to a specific value between 0 and 20

/api/v1/settings/
----------------
/api/v1/settings/restart			GET		JSON object														Performs a reboot of the microcontroller (after waiting 5000ms)

